(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(D2-K)")
	(net 3 "+9V")
	(net 4 "Net-(R1-Pad2)")
	(net 5 "Net-(R3-Pad2)")
	(net 6 "Net-(R5-Pad2)")
	(net 7 "Net-(D1-K1)")
	(net 8 "Net-(D1-K2)")
	(net 9 "Net-(J8-Pin_1)")
	(net 10 "Net-(J3-Pin_1)")
	(net 11 "Net-(J3-Pin_2)")
	(net 12 "Net-(D1-A1)")
	(net 13 "Net-(D1-A2)")
	(net 14 "Net-(J8-Pin_2)")
	(net 15 "unconnected-(RV3-Pad6)")
	(net 16 "unconnected-(RV3-Pad3)")
	(footprint "__MY_PARTS__:LEDx2_THT_5503007002F"
		(layer "F.Cu")
		(uuid "092a7ca9-0e2d-4e33-8353-6b164141d877")
		(at 83.82 60.96)
		(property "Reference" "D1"
			(at -2.54 -1.9 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c2e9212c-e450-4bdd-a908-abea82762903")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.175)
					(bold yes)
				)
			)
		)
		(property "Value" "5503007002F"
			(at -2.54 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "92d711e2-b9dd-4273-86ca-8c991482e04f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/dialight/5503007002F/2429686"
			(at -2.54 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44e77030-2752-4f77-b64c-4bcf4b4a3552")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Dual LED, cathodes on pins 2 and 4"
			(at -2.54 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "25d18af6-f309-4383-92f2-7014bf53128f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/d5e8a504-c600-49f6-bf78-101fe22e6378")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr smd)
		(fp_rect
			(start -6.35 -8.89)
			(end 6.35 3.81)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "174d2f30-301a-4df3-a40b-8b953ced7bc7")
		)
		(fp_rect
			(start -6.35 -8.89)
			(end 6.35 3.81)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "a9084feb-70af-43dd-97ca-02d62865c60a")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A1)")
			(pinfunction "A1")
			(pintype "input")
			(uuid "9b91d17d-e64b-413f-b2d7-c8ba18e8a49e")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-K1)")
			(pinfunction "K1")
			(pintype "input")
			(uuid "bc5c637b-a648-47e5-af2a-3ea66407ae69")
		)
		(pad "3" thru_hole circle
			(at -2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D1-A2)")
			(pinfunction "A2")
			(pintype "input")
			(uuid "daab5d13-3742-4e28-897c-7f8afc981856")
		)
		(pad "4" thru_hole circle
			(at -5.08 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D1-K2)")
			(pinfunction "K2")
			(pintype "input")
			(uuid "4bf29a12-3de3-484c-9c83-0a184f94da34")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_1210.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.55 0.55 0.55)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "__MY_PARTS__:Breakout1x2"
		(layer "F.Cu")
		(uuid "127c577c-2ccb-4c06-a66c-67d11fbcc5b6")
		(at 88.9 66.04 180)
		(tags "Test, Pin")
		(property "Reference" "J4"
			(at 1.27 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "021897c7-dda8-42ba-9d26-67e1a500e897")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.27 1.875 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a6fad19-9740-4ecc-9177-94f47448f0db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "049cb96c-646f-40b0-9163-0740e131e520")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01b55645-520a-4e52-b5dd-b512cecf6fc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/08b832d5-4c85-47e7-a4f3-52ee6730038c")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_poly
			(pts
				(xy -1 -1) (xy 3.54 -1) (xy 3.54 1) (xy -1 1)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "28219918-8edd-411b-a109-85b7b37965e8")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "619bc0af-50f8-45d4-a110-45fd3ca689d0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "5d507505-f881-4110-893c-92c30a9a5171")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D1-A2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "6398b468-5018-4e98-923d-cdacaa7a8769")
		)
		(embedded_fonts no)
	)
	(footprint "__MY_PARTS__:DualPotSW"
		(layer "F.Cu")
		(uuid "1747321a-e6ba-4651-8483-1da482540757")
		(at 55.88 66.04 -90)
		(property "Reference" "RV3"
			(at 0 -5.58 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "32ff19df-5285-41f0-ba74-63c28ccd6ba1")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "~"
			(at 0 -4.08 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd6fa3b0-5542-4b33-8eca-a0e87c1c18f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 -5.079999 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32255070-e722-4612-ad89-fb486c85f6a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 -5.079999 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "706ebf65-4c93-4ba0-8747-9f89a2521403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/613d3c3e-3f77-4556-a613-9d6aa04b7e74")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr smd)
		(fp_poly
			(pts
				(xy -5.08 -8.89) (xy 5.08 -8.89) (xy 5.08 6.350001) (xy -5.08 6.350001)
			)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "4ff4a3fd-f1c9-44cf-91e3-3c43ba403125")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.579999 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c4cf06c6-55d0-46e0-9a4c-e706b8c45650")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -2.54 -7.62 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J8-Pin_2)")
			(pintype "passive")
			(uuid "11776fe5-aa65-40cd-b33e-f97ab386e1e5")
		)
		(pad "2" thru_hole circle
			(at 2.54 -7.62 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+9V")
			(pintype "passive")
			(uuid "b4162f44-81a1-4cb4-911f-948cec754754")
		)
		(pad "3" thru_hole circle
			(at -2.54 0 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(RV3-Pad3)")
			(pintype "passive")
			(uuid "df7b8b80-2ae8-4770-b6e6-b194b3132cf0")
		)
		(pad "4" thru_hole circle
			(at 0 0 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pintype "passive")
			(uuid "4ba33713-d6ed-4cc0-a5e7-12168e35fc38")
		)
		(pad "5" thru_hole circle
			(at 2.54 0 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(R1-Pad2)")
			(pintype "passive")
			(uuid "a49725e7-5c24-4d4b-b066-c8b827d11e42")
		)
		(pad "6" thru_hole circle
			(at -2.54 2.54 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(RV3-Pad6)")
			(pintype "passive")
			(uuid "63b2ce79-52cd-4ac1-87c2-9b297d12f582")
		)
		(pad "7" thru_hole circle
			(at 0 2.54 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_2)")
			(pintype "passive")
			(uuid "e7221a0d-4f62-475b-b962-d2e41c2f0e2f")
		)
		(pad "8" thru_hole circle
			(at 2.54 2.54 270)
			(size 1.9 1.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(R3-Pad2)")
			(pintype "passive")
			(uuid "db03808e-9d96-4148-b4e2-508444ae2e44")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(uuid "20002777-f10d-417a-b907-67f3537a426f")
		(at 76.2 63.5 180)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 2.54 -3.56 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "790cf1c7-223e-40a4-b4b3-e72e74aac38b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2N3904"
			(at 2.54 1.27 0)
			(layer "F.Fab")
			(uuid "7d7c94cd-cef4-4fbd-8ed8-b39ca8feedff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "74c45f43-b25d-4c28-8810-b823423b1bb0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af8496ca-76d8-4957-b228-c11bb309f7b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?92*")
		(path "/fc774290-9b71-417a-a451-49729cd02227")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.74 1.850001)
			(end 4.34 1.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8b99767-d84c-4ba0-be1d-1557c2e63742")
		)
		(fp_arc
			(start 4.864184 1.122794)
			(mid 4.633903 1.509328)
			(end 4.34 1.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f19c69d-dada-435b-a54d-8e90945a707f")
		)
		(fp_arc
			(start 2.54 -2.6)
			(mid 3.936979 -2.192818)
			(end 4.896401 -1.098807)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b622b1f3-a185-4d52-bac6-43d6c72b148f")
		)
		(fp_arc
			(start 0.74 1.850001)
			(mid 0.446097 1.509328)
			(end 0.215816 1.122795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d38f8e5-3b4d-4bd1-87fb-f76065a088ed")
		)
		(fp_arc
			(start 0.1836 -1.098807)
			(mid 1.143021 -2.192817)
			(end 2.54 -2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12021476-5b27-4111-806c-2e78e7340724")
		)
		(fp_line
			(start 6.09 2.01)
			(end 6.09 -2.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7278f807-cb7b-4ab8-b1c0-774509eb90f7")
		)
		(fp_line
			(start 6.09 2.01)
			(end -1.01 2.01)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f45b4a67-18fe-4488-9686-49b477962525")
		)
		(fp_line
			(start -1.01 -2.73)
			(end 6.09 -2.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cb1da94-9102-4673-bcc2-61c5bf0e8a6b")
		)
		(fp_line
			(start -1.01 -2.73)
			(end -1.01 2.01)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "766b38cb-f5e1-45cb-9bc1-b520ca13e66c")
		)
		(fp_line
			(start 0.8 1.749999)
			(end 4.3 1.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "773e9c04-2620-460a-a2f0-627fbbd8c163")
		)
		(fp_arc
			(start 2.54 -2.48)
			(mid 4.831221 -0.949055)
			(end 4.293625 1.753625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c01a612-049d-4b82-935c-668264d1de5f")
		)
		(fp_arc
			(start 0.786375 1.753625)
			(mid 0.248779 -0.949055)
			(end 2.54 -2.48)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "186d2cb0-0038-41f3-86f1-ca049ee75510")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(uuid "96ee1162-4c8f-40df-a38f-d3537a929a1b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D2-K)")
			(pinfunction "E")
			(pintype "passive")
			(uuid "325454d6-0719-4d1e-994a-1e9b150a1950")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J8-Pin_1)")
			(pinfunction "B")
			(pintype "input")
			(uuid "bfd4d0e9-207e-41f9-843c-87ec0f0f7295")
		)
		(pad "3" thru_hole circle
			(at 5.079999 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J8-Pin_2)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "d54f4565-95eb-4ca5-bd73-529c06368c6a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "__MY_PARTS__:Breakout1x2"
		(layer "F.Cu")
		(uuid "23162eb1-7abc-4182-8dd9-951a80535e84")
		(at 63.5 58.42 180)
		(tags "Test, Pin")
		(property "Reference" "J3"
			(at 1.27 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b7b544af-3932-4f6e-b953-7c2c48a1fab7")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.27 1.875 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a489253b-42ac-425a-8494-4e3c0cf44fa0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6760aa5b-01a6-46fa-8bdd-e6b49fdf6bcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff07c1be-60fe-4610-a38c-3ebfcebccb62")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/6045d218-b70f-4212-9941-a387773ea798")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_poly
			(pts
				(xy -1 -1) (xy 3.54 -1) (xy 3.54 1) (xy -1 1)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "02502f02-ba4b-4b7f-bc21-ca68e9fce539")
		)
		(fp_text user "${REFERENCE}"
			(at 1.270001 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "509f67bc-c8a0-42c8-96b1-7008a1967b22")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "453a783f-9797-4ab1-bb2b-ed11db75ee7f")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "511a7d58-fdd9-4795-8ec9-46a37e6d758c")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "24b3ea60-2504-47ec-afde-f74aadc840d2")
		(at 78.74 68.58 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D2"
			(at 3.81 -2.12 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0c07e785-cdce-4db2-b76e-9690da982b76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1N5817"
			(at 3.81 2.12 0)
			(layer "F.Fab")
			(uuid "3a59ef44-ff21-411e-a881-cac5155e05bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3758fd54-df1d-4494-bbb2-40b9de6e5be5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fdf6d54f-8160-4216-bd8f-8c299de7f3bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/55a8c37c-7f22-4f34-bf58-6b538f153f4f")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.580001 0)
			(end 5.93 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c28ef834-c0e8-4081-81ba-d21cd94ee02c")
		)
		(fp_line
			(start 5.93 1.12)
			(end 5.93 -1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f2a4b44-66d9-4612-a0f1-eeabdc17ef52")
		)
		(fp_line
			(start 5.93 -1.12)
			(end 1.69 -1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4399e8fc-e5b0-4e17-b365-24890f146925")
		)
		(fp_line
			(start 2.53 -1.12)
			(end 2.53 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50194a43-4dd1-4975-a506-7e056798c92b")
		)
		(fp_line
			(start 2.41 -1.12)
			(end 2.41 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6de61c0a-c2d1-404d-baf9-de371bb14e1e")
		)
		(fp_line
			(start 2.29 -1.12)
			(end 2.29 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac9a1544-1881-4960-8a3e-51fd66702ce1")
		)
		(fp_line
			(start 1.69 1.12)
			(end 5.93 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "669bfa09-93a1-436d-b513-59c13f05bff3")
		)
		(fp_line
			(start 1.69 -1.12)
			(end 1.69 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b94cdf17-6b90-4cd1-a4b7-c4ad73115060")
		)
		(fp_line
			(start 1.04 0)
			(end 1.689999 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6dc44f3f-b6a8-4b72-901d-da31827fff40")
		)
		(fp_line
			(start 8.67 1.25)
			(end 8.67 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e527b24-9aab-4ff1-8ec3-08557b1296bc")
		)
		(fp_line
			(start 8.67 -1.25)
			(end -1.050001 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f488cd9-19fd-4119-8125-fc6895e50ce6")
		)
		(fp_line
			(start -1.050001 1.25)
			(end 8.67 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd031883-578e-449d-96e3-4404142074f5")
		)
		(fp_line
			(start -1.050001 -1.25)
			(end -1.050001 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "feecfc3a-c792-4ba3-bcf0-d0a5f36f5631")
		)
		(fp_line
			(start 7.62 0)
			(end 5.809999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1426282-c9af-40dd-b5e9-caa84fce96cd")
		)
		(fp_line
			(start 5.81 1)
			(end 5.81 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58d7dea4-a62c-48ee-be2b-0bb2a1ef3397")
		)
		(fp_line
			(start 5.81 -1)
			(end 1.81 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "443697e7-0811-4c63-acb3-fa6e118190df")
		)
		(fp_line
			(start 2.51 -1)
			(end 2.51 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e4fbe40-8089-4f41-902c-98400637e29f")
		)
		(fp_line
			(start 2.41 -1)
			(end 2.41 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6709d08b-d306-4e35-8d22-51b989b627aa")
		)
		(fp_line
			(start 2.31 -1)
			(end 2.31 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "190f27c3-a92b-4424-8145-13ec43703fc7")
		)
		(fp_line
			(start 1.81 1)
			(end 5.81 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8909c3b-41bd-413d-ba95-6da28062af6e")
		)
		(fp_line
			(start 1.81 -1)
			(end 1.81 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0af703e3-6d80-4e42-8c68-67372ac39054")
		)
		(fp_line
			(start 0 0)
			(end 1.81 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a37769d-865d-4be3-aa37-0e77f2d65030")
		)
		(fp_text user "K"
			(at 1.27 1.27 0)
			(layer "F.SilkS")
			(uuid "328ecb6e-c7c6-4054-bb6a-e929a11bde89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "K"
			(at 1.27 0 0)
			(layer "F.Fab")
			(uuid "59f1109d-dd4f-451e-ba5a-62dfbd126fd6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 0)
			(layer "F.Fab")
			(uuid "f3ec42f4-62d2-428a-a67f-d70ce1215cdc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "984020c4-5027-473e-97c2-e5d88538f473")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "884c8146-dfd1-47a4-8666-a8aafb25739b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "__MY_PARTS__:Breakout1x2"
		(layer "F.Cu")
		(uuid "363aaeda-b220-4f1b-a3e8-0fba789b41bc")
		(at 66.04 68.58)
		(tags "Test, Pin")
		(property "Reference" "J10"
			(at 1.27 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "59d60be9-a6be-4b5a-b0d1-4d1d777828fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.27 1.875 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "026ffee9-77a2-4a09-b925-e6c14b5dd4fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c5344a8-2f4f-4b43-acf2-03db1a001029")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2fdac9ba-0458-4c23-a581-32c27557554e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/856e3403-6759-4d52-ba83-ce405b43db31")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_rect
			(start -1 -1)
			(end 3.54 1)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "bf9fa3e5-6725-41d5-9c0b-692960118d68")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "0726e80f-57af-4f82-acb1-d68132a11a46")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+9V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "1bcdfd1d-a1b9-4dbc-9cae-9e7e691df278")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "e45db409-b298-4e2f-b664-5de5df88b8f2")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "3d37b366-67ea-474f-9d47-86f79fd56c5c")
		(at 60.96 53.34 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c579fecb-7f6d-4936-839f-087e1b3c7997")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 3.81 0 0)
			(layer "F.Fab")
			(uuid "56350b20-823f-4014-8511-d14498b6a063")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0606d1d2-e1c0-4436-b4d2-3fe9c8ea211a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "04015000-6cff-4497-98db-0643ffacdfeb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/36570c9b-75bc-4fa1-8e89-01a079d56a71")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd48820a-9b39-4055-a43a-7c1d3cbfb65e")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea99971b-e3fb-462a-b26d-00e2964afa8f")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b58bbe4-8ca0-44fd-90fc-d6607d9b2a9d")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8dd03836-2918-4cb5-b795-e521d82c3b4d")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9dd3db1-8721-4acb-be3c-54c032edae4a")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c81fd93b-ad66-452a-863f-9f6aaca158de")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29fec53a-acb6-43b9-b103-d15ba2586141")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ad9fae2-64c8-4193-b890-9191012ffbff")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "502663b1-d6c3-4f08-b375-892a113ef263")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e3b053e-b1a4-416f-8ad1-6785322d5b80")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c05347c3-1724-4f70-a832-c773d9d5e54a")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f3be698-2737-4856-b164-bbee6c09e9f0")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e92e5cec-52f5-416f-a4e9-15de765156b9")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eef049ec-8736-42f3-b219-39c0c5b506ac")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2bdb1d2-4369-44ce-9692-af8d2803ed90")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca7f62ae-ac46-4dbd-a925-682b75875b78")
		)
		(fp_text user "${REFERENCE}"
			(at 6.96 1.25 0)
			(layer "F.Fab")
			(uuid "29830ffc-48e6-4111-9215-1fac768b4fd8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(uuid "47d7d78e-8cd9-4ad3-bcec-d14e86724172")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(R3-Pad2)")
			(pintype "passive")
			(uuid "c1ff89aa-cc60-40c5-a006-ff749551e75c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "40284b38-916a-4348-913e-6ee110da3478")
		(at 78.74 71.12 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ab531235-c56c-467a-bd5e-1c19e0e882c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "240"
			(at 3.81 0 0)
			(layer "F.Fab")
			(uuid "b8b925a8-0a30-4842-a311-3fdfb6526d8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9f02c5a-4178-44bb-b9c0-f1f4f8e07a48")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0119243-eb4f-4d9f-8d71-38a2a8c30d6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/07e68212-2980-4d8d-8e4b-83495b9b356d")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "359cd8f5-931c-45a5-884e-0c53e8e24bb1")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cf0b5ad-1235-4dda-9709-087c597b3b23")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6288de9f-ff0e-4e23-8387-aa21c3c4a563")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17577537-896d-4b98-99ae-84aabe5b5187")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0b1537d8-9403-4280-b97a-b80350d48fe0")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "241380ab-54ae-439a-9c0c-4c6ea19fb923")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f5b9863-42e1-41f8-b3a2-8ad62c123c13")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ad5729d-8e73-4db4-adbc-6ffcd661a9d1")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2077b2f-8d99-4822-ad3c-0d6e5c39485a")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be4c5322-cf94-44d1-9aba-d7c4977850b9")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78b8cb77-4ee4-46d4-9f8c-83501fc7c06e")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "429b18d5-71ed-4ad4-9d52-3664ac18eab0")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b336c97-87ae-410d-9033-4eea95dc54df")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6696a233-ef63-405a-b923-e69b60f084e8")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62528fd3-f8ce-4261-9161-d419eee719c7")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d6b692f-2d14-4014-a1cd-5d52f550c998")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 -1.27 0)
			(layer "F.Fab")
			(uuid "e5444ff0-afa5-4582-850e-bf61c71807ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(R5-Pad2)")
			(pintype "passive")
			(uuid "0aea6a10-deb1-472f-8693-e93b98ed07d3")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(uuid "91f90e74-e237-4a6c-b03b-3f0e8125bc2c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "4df927fd-f94e-4826-aa6c-961fdccd7d66")
		(at 88.9 68.58 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "be85b02f-b3d7-405a-b4b7-f3cf8e18a87e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 3.81 0 0)
			(layer "F.Fab")
			(uuid "65813a5e-8aab-43b3-9673-0641228e8788")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a43afdb-0fca-4cce-b327-598def80a4e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54723de1-1b54-4eb4-acd3-70f4512f6e1a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/95ff4d7b-f97a-4e0d-bd21-261189941e5e")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6986ac6c-cad4-4edc-b639-2679c14574e9")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d30593a-ab94-4b36-8a22-1477a9f7f12f")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8dd4f936-bcb1-46c9-929b-0ff5d720767d")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6423327-594a-48eb-ac2f-698cf05c07d3")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49cdd0c1-df4d-40b4-97e1-6234ffb008bf")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd98f135-ac46-4a3e-9361-fb5e7b3212a6")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "509973b4-3281-429b-aaf7-0dc46685e3ef")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfeed0bc-f6c5-4533-94fc-2f3c549f6f2b")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5a19153-4396-4113-8f1c-02e7aa14d7ad")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86521587-c5e6-40e1-a0e4-592b9928d23d")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "851a033f-356f-400c-a2c5-1a3bc38a8adc")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "265f8bd3-bc4e-4a89-9840-5ff4c9b264fb")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3306fb33-81df-4f13-be41-26b44d635f66")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "546acff4-b249-4803-a9cb-b2fca77bab28")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3148aae3-e8f8-4d27-b496-0d5f33767341")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be184051-d7ce-4585-af23-19a08226be30")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 1.27 0)
			(layer "F.Fab")
			(uuid "3d45c63e-7016-4c31-aacb-06d9594be94d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D1-K2)")
			(pintype "passive")
			(uuid "3bde4d06-f672-44d7-914f-fde1904df07e")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(R5-Pad2)")
			(pintype "passive")
			(uuid "8e21d645-3d38-4dcd-97d6-637849e31029")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "__MY_PARTS__:Breakout1x2"
		(layer "F.Cu")
		(uuid "5653486e-e56b-40af-9c23-ea12f4616cd7")
		(at 68.58 63.5 180)
		(tags "Test, Pin")
		(property "Reference" "J8"
			(at 1.27 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "d2b72cea-3cbe-463a-9134-e3cf16623e53")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.27 1.875 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d0af496-3882-40c9-bdf6-84ca20f90eba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "731a1269-5db8-491c-b9c8-2a423c4a35f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5b4333a4-6015-4416-a9c6-232eba45626b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/9c19ef88-a262-4e3d-8210-e196c82047df")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_poly
			(pts
				(xy -1 -1) (xy 3.54 -1) (xy 3.54 1) (xy -1 1)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "e40a9d33-83c7-4b77-9570-b1e78013455f")
		)
		(fp_text user "${REFERENCE}"
			(at 1.270001 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "b2480c4b-603b-4aff-b67c-7a58341ddef8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0c3c35a9-30fd-47b2-807d-d7ba092f5879")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "01b3ead6-e0dc-4033-bed3-f43075aa0309")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "9e87cbf7-7f1a-443e-9baa-efde46ae8ecf")
		(at 53.34 55.88)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0df29ce2-ac46-4708-83c6-fa394f6ff76c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 3.81 0 0)
			(layer "F.Fab")
			(uuid "3e454c4a-d0ec-49b6-96dd-910605f0c0cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65c97776-b16b-4474-bc81-7771a75c7c25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b7136da-c128-462a-9feb-7613ad666981")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/bd30ed5b-eb3a-4a9e-a1b2-3df2f8c8f123")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "447c3df1-c0ae-4fce-9291-5a6ae23baa95")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6925c996-8778-410f-adef-bd40b13be25b")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b557cd6-8613-4193-bbe3-8e2f18bda62c")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1952778e-60f9-4277-b3de-70754a707ebc")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68c028fd-87b8-4404-ae63-eea0830c89c9")
		)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d0f595d-b7ec-4f9e-ab9d-1fe856447d3a")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8196268e-924e-4578-98e3-40f133ce96b2")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fa9995a-b4fd-4cfe-9dad-c18d822549a9")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5ee16c1-7712-49f1-8511-3289af8af44f")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24f5289f-20f7-4beb-b486-d8c7f13e83ba")
		)
		(fp_line
			(start 0 0)
			(end 0.66 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a74bacc-63ef-4a2a-891a-f423e350a0ae")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d078030-f413-4f69-a501-4dedcca7afa5")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f7d6cdc-08ac-471f-8858-d807f96bc8e8")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32e97e20-7031-483a-b167-0bbb2bea948e")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc43c435-44a9-40f4-87d3-233704e31c96")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23fde84b-b954-44e4-94b6-1f7778a3deed")
		)
		(fp_text user "${REFERENCE}"
			(at 0.66 -1.25 0)
			(layer "F.Fab")
			(uuid "faca33e6-0dff-4cdf-b804-339a729d1ccb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(R3-Pad2)")
			(pintype "passive")
			(uuid "e70b87b5-9c21-4cb0-814e-1c45f84a15c1")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_2)")
			(pintype "passive")
			(uuid "662208e7-a3e1-4e7a-8b3c-86fb861841d5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "a43962de-8322-4131-ab1a-52c829eafdaf")
		(at 88.9 71.12 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e27d0136-6c14-4fb2-a47c-8a033ca0593a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "120"
			(at 3.81 0 0)
			(layer "F.Fab")
			(uuid "3c38585c-8a34-42af-b9a2-6a964dd6ce9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5cdc453-d631-4c32-9f38-545c31a69a0f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "62af4f5b-33d4-4e3b-818e-1823ce5be590")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/56dba174-6ccb-4654-8e92-fda70bd70ba2")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94e337ab-0d36-4b5a-95c0-7d57b4ebb8eb")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9dbeb14-70e0-4a12-8a40-847cd5176a88")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17bc734e-4b99-4abd-a2d4-09dc6a550ee4")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b58d787a-7174-4fe2-bb94-63b7f7592b5d")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ecdfce4-f1dd-4bf9-90a5-541addc8cb8e")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a1b60ab-2d7c-4e40-9550-c135ad4c0c69")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef5fb17d-ea80-498d-a7d1-740fc37e154f")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49af5ddc-d06b-4f61-9631-6cf7c9aa634d")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e0eef91-a6a0-453d-9d12-08a71be3d389")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c7752fe-6db9-487f-bc8a-dfb65dd16b02")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a795e07e-64f9-4885-a3a9-73222276af8b")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe714234-becc-42e8-847f-b3c38887adb3")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7bc6ebf3-0cdf-40cd-bc3d-c0195fc38f24")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afce3fa6-a59e-4b17-a8bd-464938fce7d0")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad8e7224-a91b-4739-9fe7-14d00530cf6e")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a6d9da3-6a8f-40bd-a04e-7cbf1065d398")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 1.27 0)
			(layer "F.Fab")
			(uuid "c37fcd81-3215-4039-9a32-61be44e3ac13")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-K1)")
			(pintype "passive")
			(uuid "6cc07aff-8752-4a3c-8d6a-42a3e609f25b")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(R5-Pad2)")
			(pintype "passive")
			(uuid "55d34509-3c5a-4baf-a379-e80d69950f44")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(uuid "c3c258c5-042d-4afc-998a-713021bbbd68")
		(at 73.66 58.42 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 1.25 -4.4 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "177be861-fc18-488b-8b4f-cc75050ab8ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220μ"
			(at 1.25 2.54 180)
			(layer "F.Fab")
			(uuid "467f8e56-81a0-47a3-82f5-c0ca30ba965c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e6d32ac-2f95-4023-b66d-587b1075bd8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd606e7a-d0ff-40f5-b5fe-4c1dac1de426")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/0b06aa28-4995-4176-a459-67b21d6c6083")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 -3.23)
			(end 1.33 3.23)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f3586fc-7c26-4446-8065-00fd4d10feff")
		)
		(fp_line
			(start 1.29 -3.23)
			(end 1.29 3.23)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28e11145-f8aa-447e-82c1-e71ee527f632")
		)
		(fp_line
			(start 1.25 -3.229999)
			(end 1.25 3.229999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "269b8cbf-a60d-42fd-992c-bfc4aa0a0650")
		)
		(fp_line
			(start 1.37 -3.228)
			(end 1.37 3.228)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "519d8544-42bb-4b21-b590-dd88654e831f")
		)
		(fp_line
			(start 1.41 -3.227)
			(end 1.41 3.227)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f378ae4-8120-4484-b1b2-d92d14ca8b6e")
		)
		(fp_line
			(start 1.45 -3.224)
			(end 1.45 3.224)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd9e4f01-d99c-4dc3-a967-fc148aba1048")
		)
		(fp_line
			(start 1.49 -3.222)
			(end 1.49 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61a2678e-7df7-4806-a54f-72d5d02e7097")
		)
		(fp_line
			(start 1.53 -3.218)
			(end 1.529999 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a58c9231-874c-4348-b654-35e15693eeb1")
		)
		(fp_line
			(start 1.57 -3.215)
			(end 1.57 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e85081c4-7175-4932-aa1d-791a62ffa8af")
		)
		(fp_line
			(start 1.61 -3.211)
			(end 1.61 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a2c5c6c-09f3-46e4-b39d-7f7859ad87c6")
		)
		(fp_line
			(start 1.65 -3.206)
			(end 1.65 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b1393b0-053c-4efb-940e-386aa044fd00")
		)
		(fp_line
			(start 1.69 -3.201)
			(end 1.69 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "454fea4e-20c7-4664-9244-1fbec9c61604")
		)
		(fp_line
			(start 1.73 -3.195)
			(end 1.73 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c871640f-49dd-4288-8cf9-18ec0559d69f")
		)
		(fp_line
			(start 1.77 -3.189001)
			(end 1.77 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4022c01c-ea73-44ff-9c32-f3cb42ae369e")
		)
		(fp_line
			(start 1.81 -3.182)
			(end 1.81 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc7817d4-93c8-49dd-8da8-348af5e9a655")
		)
		(fp_line
			(start 1.850001 -3.175)
			(end 1.85 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "727e9329-a8cf-44c2-ad49-c982d6d7d4c1")
		)
		(fp_line
			(start 1.89 -3.167)
			(end 1.89 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "733d13f0-413d-4a23-8d82-19d8180173bc")
		)
		(fp_line
			(start 1.93 -3.159)
			(end 1.93 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a42ba02-ba2d-457d-a1b7-cbe5f75d3dd8")
		)
		(fp_line
			(start 1.971 -3.15)
			(end 1.971 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6d52528-813f-47fd-86e2-8189784f9d8c")
		)
		(fp_line
			(start 2.011 -3.141)
			(end 2.011 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4a54c79-cd1d-42b1-9acd-6e76c068591c")
		)
		(fp_line
			(start 2.051 -3.131)
			(end 2.051 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a2f221e-7476-4f9a-9cd1-2aec2ab45adc")
		)
		(fp_line
			(start 2.091 -3.121)
			(end 2.091 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a8ee4e6-f8ee-46d9-b0ac-37122330060b")
		)
		(fp_line
			(start 2.131 -3.110001)
			(end 2.131 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab2d8610-aaca-42b3-8d32-64959ae31075")
		)
		(fp_line
			(start 2.171 -3.098)
			(end 2.171 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9416cc3-1294-45e6-ab3a-4070612e07d4")
		)
		(fp_line
			(start 2.211001 -3.086)
			(end 2.211 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e847926-03cd-4dc3-abac-150ea2c7974b")
		)
		(fp_line
			(start 2.251 -3.074)
			(end 2.250999 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e128d21-dd37-4f25-bceb-b035fde65c89")
		)
		(fp_line
			(start 2.291 -3.060999)
			(end 2.291001 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cc01cd7-921f-4fc1-a91d-67a6ca7456a0")
		)
		(fp_line
			(start 2.331 -3.046999)
			(end 2.331 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b9a03c9-21fd-41cf-bb9a-bd1138951e05")
		)
		(fp_line
			(start 2.371 -3.033)
			(end 2.371 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad5c09e5-35ce-44b1-9f38-fe917afe8e0a")
		)
		(fp_line
			(start 2.411 -3.018)
			(end 2.411 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73cf0513-01b4-405e-8c9d-7bc8e6558f05")
		)
		(fp_line
			(start 2.451 -3.002)
			(end 2.451 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ca6d85e-bdf7-4ac8-b349-8cd4a5f5577a")
		)
		(fp_line
			(start 2.491 -2.986)
			(end 2.491 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3888553-0cbb-4915-b482-b96be580666d")
		)
		(fp_line
			(start 2.531 -2.97)
			(end 2.531 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7c13d68-113b-4120-8258-6b7daaed39fb")
		)
		(fp_line
			(start 2.571 -2.952)
			(end 2.571 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19bbb170-2b9d-4f75-aa55-db951d0d349f")
		)
		(fp_line
			(start 2.611 -2.934)
			(end 2.611 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64b16a5e-d336-429c-ab24-8f6fddd0a9e6")
		)
		(fp_line
			(start 2.651 -2.915999)
			(end 2.651 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1df26b6-7a9d-4912-949c-b4f9939740ff")
		)
		(fp_line
			(start 2.691 -2.896)
			(end 2.691 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a918b18f-e75b-485e-bb8c-dc40a3b989c4")
		)
		(fp_line
			(start 2.731001 -2.876)
			(end 2.731001 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5767bcda-094c-4294-9695-18dc69e38b0a")
		)
		(fp_line
			(start 2.771 -2.856)
			(end 2.771 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d97ed7e-3dad-42fb-bdfd-da9c211c906c")
		)
		(fp_line
			(start 2.811 -2.834)
			(end 2.811 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "190aaa42-51dd-444c-8d49-2b4c2cd41200")
		)
		(fp_line
			(start 2.851 -2.812)
			(end 2.850999 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46e8423a-5b19-4c91-8dc8-7df91881979a")
		)
		(fp_line
			(start 2.891 -2.79)
			(end 2.891 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b02dd63-3f9d-4853-8bae-a3773f6edb7d")
		)
		(fp_line
			(start 2.931 -2.765999)
			(end 2.931 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fdb79933-dffc-47ae-9b03-c631b3be9509")
		)
		(fp_line
			(start 2.971 -2.742)
			(end 2.971 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65c24df3-c853-4a31-ba9f-8ab2663e7300")
		)
		(fp_line
			(start 3.011001 -2.716)
			(end 3.011 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ee690e4-bc44-43b8-96a7-bdeb402e15c9")
		)
		(fp_line
			(start 3.051 -2.69)
			(end 3.051 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1731624-190b-4161-bda1-37fb888fb9b0")
		)
		(fp_line
			(start 3.091001 -2.664)
			(end 3.091 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3186611a-8dfc-41dc-b530-691aa12ebe75")
		)
		(fp_line
			(start 3.131 -2.636)
			(end 3.131 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02a85307-df5a-4c8d-ab0f-c136b493d4e6")
		)
		(fp_line
			(start 3.171 -2.607)
			(end 3.171001 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92790554-a79d-4915-bfc1-f816e036f55f")
		)
		(fp_line
			(start 3.211 -2.578)
			(end 3.211 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff9330f4-5405-49c5-b368-be4b0a9d78ad")
		)
		(fp_line
			(start 3.251 -2.548)
			(end 3.251 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d09180e-0fdd-4344-bb10-4de2d768c72c")
		)
		(fp_line
			(start 3.291 -2.516)
			(end 3.290999 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4780cf4-99c9-4397-817e-b45de40381a9")
		)
		(fp_line
			(start 3.331 -2.484)
			(end 3.331 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04d50426-d6a8-4307-b12e-7cd1f2de7619")
		)
		(fp_line
			(start 3.371 -2.450001)
			(end 3.371 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c36cf7ed-4dc2-4be1-973f-16b2365c836b")
		)
		(fp_line
			(start 3.411 -2.416)
			(end 3.411 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "401e9231-c69c-4ef9-88fc-cfb5d0d403ff")
		)
		(fp_line
			(start 3.451 -2.380001)
			(end 3.451 -1.040001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "266e0751-a5de-43ec-aaa1-607cadab8b1d")
		)
		(fp_line
			(start 3.491 -2.343)
			(end 3.491 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a26bb6a-d8da-40b4-972a-e9b897db0d4a")
		)
		(fp_line
			(start 3.531 -2.305)
			(end 3.531 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82107772-33f5-4ad6-8cf8-17a44bf82d43")
		)
		(fp_line
			(start 3.571 -2.265)
			(end 3.571 2.265)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d0ba588-d993-45e4-81f4-806a01281eb7")
		)
		(fp_line
			(start 3.611 -2.224)
			(end 3.611 2.224)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2d13b8c-1d89-481e-b487-fa740a89ce14")
		)
		(fp_line
			(start 3.651 -2.182)
			(end 3.651 2.182)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d18228e1-7e8f-4582-815f-c745aa3512eb")
		)
		(fp_line
			(start -1.935241 -2.154)
			(end -1.935241 -1.524)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b44834c0-3615-4903-85be-d786abbd6871")
		)
		(fp_line
			(start 3.691 -2.137)
			(end 3.691 2.137)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d1b61eb6-9e8c-4edc-9b56-b091717504ee")
		)
		(fp_line
			(start 3.731 -2.092)
			(end 3.731 2.092)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92e5437d-91bc-4639-8be3-948ef2ca6e42")
		)
		(fp_line
			(start 3.771 -2.044)
			(end 3.771 2.044)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cad1aa0-8f53-4deb-8cd5-5849d6e916a6")
		)
		(fp_line
			(start 3.811 -1.995)
			(end 3.811 1.995)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76f0be55-4bc0-4b75-82ee-79d1619a92e8")
		)
		(fp_line
			(start 3.851 -1.944)
			(end 3.851 1.944)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aae12007-1147-4a34-9d72-fb977ea53b4e")
		)
		(fp_line
			(start 3.891 -1.89)
			(end 3.891 1.89)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e037ed2b-48c9-49ff-b4bf-4ec402f8216c")
		)
		(fp_line
			(start -2.250241 -1.839)
			(end -1.620241 -1.839)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ba0bbb3-b787-4c8a-8a4d-a13f72ae9251")
		)
		(fp_line
			(start 3.931 -1.834)
			(end 3.931 1.834)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "72989492-96e1-42da-8070-6be119ac9040")
		)
		(fp_line
			(start 3.971 -1.776001)
			(end 3.971 1.776001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c88acd4-d073-4fba-b5e2-2620ae76f03f")
		)
		(fp_line
			(start 4.011 -1.714)
			(end 4.011 1.714)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93d7d1b8-af93-4414-8628-efc1067f2b85")
		)
		(fp_line
			(start 4.051 -1.65)
			(end 4.051 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46dfda08-0119-44f1-a66d-2e91c5595e26")
		)
		(fp_line
			(start 4.091 -1.581)
			(end 4.091 1.581)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4af361f5-2ef8-4901-9906-052b1717ee74")
		)
		(fp_line
			(start 4.131 -1.509)
			(end 4.131 1.509)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83f56f14-565f-4f86-89af-a433a311fcb0")
		)
		(fp_line
			(start 4.170999 -1.432)
			(end 4.170999 1.432)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a42c0afb-15ba-48b6-8735-9a2555a1dd30")
		)
		(fp_line
			(start 4.211 -1.35)
			(end 4.211 1.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "649efa7e-2792-4f82-b92f-7c9ee26200c9")
		)
		(fp_line
			(start 4.251 -1.262)
			(end 4.251 1.262)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e77a4f8-7bfa-4ae3-af29-4c86fe138397")
		)
		(fp_line
			(start 4.291 -1.165)
			(end 4.291 1.165)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6dc87993-f24d-4340-8a54-64cd6533d1c0")
		)
		(fp_line
			(start 4.331 -1.059001)
			(end 4.331 1.059001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "427cc131-4015-497c-a917-488d1fbfc848")
		)
		(fp_line
			(start 4.371 -0.94)
			(end 4.371 0.94)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32946637-1616-463a-9f9d-2f199b02edc8")
		)
		(fp_line
			(start 4.411 -0.802001)
			(end 4.411 0.802001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a636f8c2-9c7e-4362-a72b-6ecfd31b532d")
		)
		(fp_line
			(start 4.451 -0.633)
			(end 4.451 0.633)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "315bfc4a-b703-422f-bd08-4c832abf858e")
		)
		(fp_line
			(start 4.491 -0.401999)
			(end 4.491 0.401999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ddd9c0d2-80d2-43b4-8cbc-e3b763a49d3c")
		)
		(fp_line
			(start 3.531 1.04)
			(end 3.531 2.305)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20ecaf8d-ec09-448c-9b4d-6d3613dc2c9b")
		)
		(fp_line
			(start 3.491 1.04)
			(end 3.491 2.343)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5844d22-af0f-4fb9-b21a-8b5c2726d34c")
		)
		(fp_line
			(start 3.411 1.04)
			(end 3.411 2.416)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f0f39ea-e000-45fa-aa86-b0d896f1c571")
		)
		(fp_line
			(start 3.371 1.04)
			(end 3.371 2.450001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55ba7d00-1b19-4482-8f6f-c3c804c1baa2")
		)
		(fp_line
			(start 3.331 1.04)
			(end 3.331 2.484)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f708e32f-6e1f-421c-b307-689bfb1ba8f4")
		)
		(fp_line
			(start 3.290999 1.04)
			(end 3.291 2.516)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba25999a-1b75-4b8f-82e4-740a19b8e05a")
		)
		(fp_line
			(start 3.251 1.04)
			(end 3.251 2.548)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "833f5fe2-2ae0-4e4e-b0c2-4160eb7942a6")
		)
		(fp_line
			(start 3.211 1.04)
			(end 3.211 2.578)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acc432bd-5e4d-4ebb-a347-bbf900474617")
		)
		(fp_line
			(start 3.171001 1.04)
			(end 3.171 2.607)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e32f02d-f698-4864-91cc-1910a1c17c17")
		)
		(fp_line
			(start 3.131 1.04)
			(end 3.131 2.636)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a0fa007-f0d4-4fdb-a30e-7caad420e8e2")
		)
		(fp_line
			(start 3.091 1.04)
			(end 3.091001 2.664)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0faaecde-3023-4bdf-821b-6e734ee914fc")
		)
		(fp_line
			(start 3.051 1.04)
			(end 3.051 2.69)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4636f0c-e558-48cb-8986-3e1a30b5cb6e")
		)
		(fp_line
			(start 2.971 1.04)
			(end 2.971 2.742)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da1c2a85-1748-4b2a-9259-f5b2a20df3f8")
		)
		(fp_line
			(start 2.931 1.04)
			(end 2.931 2.765999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bbb05d8-cda0-4a64-adb0-a31f003d46d4")
		)
		(fp_line
			(start 2.891 1.04)
			(end 2.891 2.79)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1a95b09-79ff-4dfa-b88b-5f5565587a6a")
		)
		(fp_line
			(start 2.850999 1.04)
			(end 2.851 2.812)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "533e38ac-f322-437d-b7a8-55bde445af35")
		)
		(fp_line
			(start 2.811 1.04)
			(end 2.811 2.834)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3222e25b-6e10-49b3-858d-e088a0e5ed3d")
		)
		(fp_line
			(start 2.771 1.04)
			(end 2.771 2.856)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc1630e7-998a-40f8-a767-7b9ff5d82cf1")
		)
		(fp_line
			(start 2.731001 1.04)
			(end 2.731001 2.876)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8483f9aa-23bf-47f8-b33f-f80a827f276e")
		)
		(fp_line
			(start 2.691 1.04)
			(end 2.691 2.896)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91517205-ff81-4e63-8aa6-0fe4f22042c4")
		)
		(fp_line
			(start 2.651 1.04)
			(end 2.651 2.915999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a187108-8bae-42b2-9759-8a81abc4e45e")
		)
		(fp_line
			(start 2.611 1.04)
			(end 2.611 2.934)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a0d9471-52b6-4eeb-8c41-999227c0a9ac")
		)
		(fp_line
			(start 2.531 1.04)
			(end 2.531 2.97)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc864984-585a-45a9-8eda-a808026e9ea6")
		)
		(fp_line
			(start 2.491 1.04)
			(end 2.491 2.986)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95c5cd0d-48f9-4b8a-9fc4-4d9409ead5a0")
		)
		(fp_line
			(start 2.451 1.04)
			(end 2.451 3.002)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76e5bcd1-5b51-494d-8b72-50c578de6523")
		)
		(fp_line
			(start 2.371 1.04)
			(end 2.371 3.033)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07cc95a2-b510-4014-b241-d9a4fe43e21b")
		)
		(fp_line
			(start 2.331 1.04)
			(end 2.331 3.046999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9f5e1d5-8184-4ff3-b53f-2ed32c41166c")
		)
		(fp_line
			(start 2.291001 1.04)
			(end 2.291 3.060999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10e39301-8d55-4e2e-b4e4-fc060573de3f")
		)
		(fp_line
			(start 2.250999 1.04)
			(end 2.251 3.074)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95ad5245-ff60-4bf2-8ebf-6d513e56f23c")
		)
		(fp_line
			(start 2.211 1.04)
			(end 2.211001 3.086)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cf7acb4-da52-4726-b776-6adfd6df9198")
		)
		(fp_line
			(start 2.171 1.04)
			(end 2.171 3.098)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "faa0a1a4-4064-4f94-9026-86c5f68e4dfd")
		)
		(fp_line
			(start 2.091 1.04)
			(end 2.091 3.121)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a25907d-cc8a-4409-9a5e-c261bf82f4e5")
		)
		(fp_line
			(start 2.051 1.04)
			(end 2.051 3.131)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9aac68c2-3b2e-4e0e-a0d8-ecd2305c89b1")
		)
		(fp_line
			(start 2.011 1.04)
			(end 2.011 3.141)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8fb0719-ddac-43a5-8977-018b2a93bd87")
		)
		(fp_line
			(start 1.93 1.04)
			(end 1.93 3.159)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87951cb9-3df0-49cc-a974-b2db5179b77a")
		)
		(fp_line
			(start 1.89 1.04)
			(end 1.89 3.167)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef483ac9-1a8d-45eb-a1cc-60aebda0c6e5")
		)
		(fp_line
			(start 1.81 1.04)
			(end 1.81 3.182)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bfaae19-4d55-4bf4-9c16-4d4d5e055e91")
		)
		(fp_line
			(start 1.77 1.04)
			(end 1.77 3.189001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad58f637-f73f-4392-af0f-3676dcb45071")
		)
		(fp_line
			(start 1.73 1.04)
			(end 1.73 3.195)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6473fecd-8d59-4c4e-a3fb-11169c9e7823")
		)
		(fp_line
			(start 1.65 1.04)
			(end 1.65 3.206)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66f67f6a-c4a9-4b69-b15c-8d9f7c1561a6")
		)
		(fp_line
			(start 1.61 1.04)
			(end 1.61 3.211)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09489db4-5e0c-44bf-b19a-e6c27ecc44e4")
		)
		(fp_line
			(start 1.57 1.04)
			(end 1.57 3.215)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cea7a602-e33a-4fad-bb97-81335bae55f6")
		)
		(fp_line
			(start 1.529999 1.04)
			(end 1.53 3.218)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ab26244-92f8-4ba9-ae24-d1109fd57c69")
		)
		(fp_line
			(start 1.49 1.04)
			(end 1.49 3.222)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd3fd598-5bd7-4911-8799-f97da6b3c9d5")
		)
		(fp_line
			(start 3.451 1.040001)
			(end 3.451 2.380001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6d9f11a-7996-4b2e-a891-ab657ea9ff3f")
		)
		(fp_line
			(start 3.011 1.040001)
			(end 3.011001 2.716)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f936fdca-0104-48fb-9afb-ac39788a435c")
		)
		(fp_line
			(start 2.571 1.040001)
			(end 2.571 2.952)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "726f3772-d48b-48d7-84f8-57a944339719")
		)
		(fp_line
			(start 2.411 1.040001)
			(end 2.411 3.018)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6d09b3f-e7d2-4dcc-9eb6-d4b4efe2d456")
		)
		(fp_line
			(start 2.131 1.040001)
			(end 2.131 3.110001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c3e3ce2-d717-4cc3-a233-6c13a4712635")
		)
		(fp_line
			(start 1.971 1.040001)
			(end 1.971 3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eba787f8-43d3-4866-8feb-d64c827ffcf3")
		)
		(fp_line
			(start 1.85 1.040001)
			(end 1.850001 3.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55274654-da19-4ac5-ae28-4a87522750d6")
		)
		(fp_line
			(start 1.69 1.040001)
			(end 1.69 3.201)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e62f3e06-091a-47d2-a5a0-de30cfcd65ab")
		)
		(fp_circle
			(center 1.249999 0)
			(end 4.52 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "bda7338b-2ab0-4c64-8f77-16aec6130e48")
		)
		(fp_circle
			(center 1.249999 0)
			(end 4.650001 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "438ebe7d-6152-4424-be92-958e1bbeb147")
		)
		(fp_line
			(start -1.128972 -1.6885)
			(end -1.128972 -1.0585)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "504d466f-c862-4ac1-bd9d-b5f05763ed03")
		)
		(fp_line
			(start -1.443972 -1.3735)
			(end -0.813972 -1.3735)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3e62391-080e-4bdf-95f5-e40c1c30d3fa")
		)
		(fp_circle
			(center 1.249999 0)
			(end 4.4 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "78b8478b-a4e8-4c61-9a1f-ad01e5603778")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 2.54 180)
			(layer "F.Fab")
			(uuid "d8541336-4ea3-4501-8e3d-75960d5055ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J8-Pin_1)")
			(pintype "passive")
			(uuid "aad57935-23fc-40bf-b9cf-4ba27a434bef")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e247d867-b9d8-4f46-855e-b557d25e881f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "c91487d3-fced-4067-aa52-da0235082818")
		(at 68.58 60.96 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "d42f2d9b-d041-4edd-ab56-bd872776bd20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.8k"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "816e0a07-2843-4249-a2aa-43e0a0ee45eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b23f9d1a-fb3e-4c11-a4be-0558bea8a727")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9f3eb4c-6dc8-4da4-84b9-76b14a5be7d9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7f2d3eb4-42cc-4e06-b086-0f751a8875af")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6c6c248-3e68-4eba-9d01-4b8f064c16af")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a9e9057-a722-44b8-9dbe-9f0e772abb51")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbbda4cd-959b-4e2d-bc93-8e7043885610")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ecf14371-8f0d-40e0-bc39-6c6cc9299dd7")
		)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f50cd5b-4a8e-4a6f-b15e-24f33b981452")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64d4dfa1-f4cc-44ac-a062-9f57226ab1ea")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4ea3c1c2-eaad-45aa-ac51-49f2f1e308f1")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a382439-a5f1-42c9-84f6-6571cba818af")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd1628d2-c641-458e-9df7-0fc848d2b5b9")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71077ac4-2407-483c-8d8f-0b1933222fd4")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0294affa-b233-4409-9e22-7b92210b6200")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "157ee8ec-a50f-4582-af90-41dae40f7940")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fe703a2-40a3-494c-818e-a6531fc1bb69")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5894affc-bf64-4306-8df5-89fb80239400")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01f0e0dd-457b-462b-b32a-e106fdeab7ac")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "483ea127-1a07-4a6a-82db-3208c0ad3528")
		)
		(fp_text user "${REFERENCE}"
			(at 6.96 1.25 180)
			(layer "F.Fab")
			(uuid "018fc6a6-da22-4c19-a9e7-21ce3dc7df4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J8-Pin_2)")
			(pintype "passive")
			(uuid "0297d450-f649-4bab-8eac-c571fa6a9fa9")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(R1-Pad2)")
			(pintype "passive")
			(uuid "51db0ce6-83ba-4be2-a91c-824d2bb52a95")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "cda8f8d3-557f-4b74-a228-6e553193fa11")
		(at 66.04 53.34 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "11b9baa3-eb45-48bd-98b8-02acd8a6dd03")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "20k"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "ef194c93-38d9-4f04-86e8-8a6b1d46a80c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9885561-3f0c-40ac-89f0-d6860762c72a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "085d60dc-725a-4263-a098-d837e2478773")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7011802b-ce88-47d4-b207-086bdefe0524")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6163ecb0-db10-45f1-adbf-de055ff376f9")
		)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7121f24-a822-46d1-b3d7-633bd5375f56")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "107bfd35-16b3-453c-a280-02aea827b5c8")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1f27232-e448-425f-82aa-a200416f60bf")
		)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "033d0aa8-7077-42b0-a8dd-cdf900c4f837")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2297e71e-3a37-447f-b511-45baad2ea67f")
		)
		(fp_line
			(start -1.05 1.5)
			(end 8.67 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c7f045c-9b52-410a-b0d6-1d2b4f33fe27")
		)
		(fp_line
			(start 8.67 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d374653-2698-4f5e-aad5-75ff80cc9cd8")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec0afa3b-427d-4eec-9b50-71c49877c4ca")
		)
		(fp_line
			(start 8.67 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "063f57bf-cbbd-4bed-b9f4-b73d5979b954")
		)
		(fp_line
			(start 0.66 1.25)
			(end 6.96 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e15f9b1a-cb39-4451-bedc-242a419d6af0")
		)
		(fp_line
			(start 6.96 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e52c52d-53bc-4c79-ac0a-3af33dfda8b4")
		)
		(fp_line
			(start 0 0)
			(end 0.659999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a095fbc-7ddd-4804-a0b1-d4f1c9dd8576")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "402d1e11-861f-4c8c-8255-b05d64264d77")
		)
		(fp_line
			(start 0.66 -1.25)
			(end 0.66 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e46a9345-7de4-4194-b93f-9deb09fc3436")
		)
		(fp_line
			(start 6.96 -1.25)
			(end 0.66 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11980b25-751d-481e-bca7-2acf76f6be96")
		)
		(fp_text user "${REFERENCE}"
			(at 0.66 -1.25 180)
			(layer "F.Fab")
			(uuid "5cd85462-1b95-4a23-8a81-0d26e3046818")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(R1-Pad2)")
			(pintype "passive")
			(uuid "45f859eb-511c-4546-85e9-c97928085dd7")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pintype "passive")
			(uuid "aacc90a9-af32-4aa5-88d0-59d5972ac565")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "__MY_PARTS__:Breakout1x2"
		(layer "F.Cu")
		(uuid "d36f00bf-128b-4a7a-8bf5-0a9cb0c1702b")
		(at 73.66 53.34)
		(tags "Test, Pin")
		(property "Reference" "J6"
			(at 1.27 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f897bbd9-3e8b-4b08-b9f9-18a87edf8e7b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.27 1.875 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "89b90e76-3d2c-44d9-9fa7-1dc27ae82c78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "396118a9-3743-40ce-82e0-ee8efa3f2347")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bc7b7aa-f4c9-43ce-a745-ef6b910c8f25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/7d9bbcd0-cdea-4797-bd4d-328f3bfd6fcc")
		(sheetname "/")
		(sheetfile "relay_fidget.kicad_sch")
		(attr through_hole)
		(fp_poly
			(pts
				(xy -1 -1) (xy 3.54 -1) (xy 3.54 1) (xy -1 1)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "85459f67-c9c1-41e7-82f4-cb2d90562edf")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "80976408-3a2d-4866-a6a6-d886b67f3413")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ca7f94c2-039a-4233-8524-c0194fdbcf1a")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D2-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(uuid "d1519165-486c-4891-a14d-552cbc597d41")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 50.8 50.8)
		(end 91.44 73.66)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "8f855ec3-9aa5-40de-8675-c7be37d93b85")
	)
	(gr_text "6"
		(at 68.58 66.04 0)
		(layer "F.SilkS")
		(uuid "20af1127-9a0c-43b5-b9cd-766547c76713")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "+"
		(at 66.04 71.12 0)
		(layer "F.SilkS")
		(uuid "238b1929-bb21-4021-a9b9-cf777431a5cd")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "120"
		(at 85.09 71.12 0)
		(layer "F.SilkS")
		(uuid "43235ab0-45a0-4685-b217-c67452e1d102")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "100"
		(at 85.09 68.58 0)
		(layer "F.SilkS")
		(uuid "450f1969-01cc-4e4c-883d-dd37f4e54e4f")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "470"
		(at 57.15 53.34 0)
		(layer "F.SilkS")
		(uuid "808c9033-6261-4c2f-b53e-bd2774be451d")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "9"
		(at 66.04 66.04 0)
		(layer "F.SilkS")
		(uuid "84acf8dd-d5e8-4762-bf7b-cca6d240206e")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "240"
		(at 74.93 71.12 0)
		(layer "F.SilkS")
		(uuid "8e8da308-0969-4987-bea8-cf1ffd4fbd42")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "5"
		(at 63.5 60.96 0)
		(layer "F.SilkS")
		(uuid "9a5f6dbf-c7c3-4381-b9e5-a5a7b6d7e976")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "1"
		(at 73.66 52.07 0)
		(layer "F.SilkS")
		(uuid "a04977aa-9c06-47ec-8c73-cd22109c2a1c")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "4"
		(at 76.2 52.07 0)
		(layer "F.SilkS")
		(uuid "ad08208e-fc25-4a2c-9b1c-5c87a3710e88")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "-"
		(at 68.58 71.12 0)
		(layer "F.SilkS")
		(uuid "b8a0d857-b344-4b50-a2ba-1cc1acbc7801")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "8"
		(at 88.9 64.77 0)
		(layer "F.SilkS")
		(uuid "c2832cf5-61d9-4d12-8881-22ad76a337f2")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "10k"
		(at 57.15 55.88 0)
		(layer "F.SilkS")
		(uuid "c8ba3fbd-d2ad-4310-bb1e-dda4289ae7b4")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "20k"
		(at 66.04 57.15 90)
		(layer "F.SilkS")
		(uuid "d5cf113c-a43a-4ec9-a6af-014d83865331")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(gr_text "7"
		(at 60.96 60.96 0)
		(layer "F.SilkS")
		(uuid "d65fa535-49fd-4987-a948-4fc77d2a2256")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "A"
		(at 86.36 64.77 0)
		(layer "F.SilkS")
		(uuid "dc8cb9ca-5ef1-4fa0-ab49-38913e15570d")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "1.8k"
		(at 68.557345 57.155205 90)
		(layer "F.SilkS")
		(uuid "f59a7599-09ed-4c78-a68c-03e3a200f438")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(segment
		(start 71.871 51.551)
		(end 62.749 51.551)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "0afd4802-e131-44a6-b1f7-c01c13146e43")
	)
	(segment
		(start 73.66 53.34)
		(end 71.871 51.551)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "2841e429-cc00-4445-b653-00e9549798f8")
	)
	(segment
		(start 68.58 68.58)
		(end 71.12 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "2b613091-78cd-4903-9e21-83d241325a66")
	)
	(segment
		(start 73.66 55.92)
		(end 74.93 57.19)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "3a75139e-7a9c-4ce1-aa3e-e6bd9978401c")
	)
	(segment
		(start 62.749 51.551)
		(end 60.96 53.34)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "54c2a287-750b-4edb-9659-9bf0c6d686b2")
	)
	(segment
		(start 74.93 64.77)
		(end 71.12 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "7ddbc089-0634-4f89-a8a9-f7202c2dd02b")
	)
	(segment
		(start 73.66 53.34)
		(end 73.66 55.92)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "c47af6f4-828d-4f0c-aa08-802d40ae3f74")
	)
	(segment
		(start 74.93 57.19)
		(end 74.93 64.77)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "c62fe710-b7a4-46d9-8981-ff0ce88b7921")
	)
	(segment
		(start 71.12 68.58)
		(end 71.12 71.12)
		(width 0.5)
		(layer "B.Cu")
		(net 1)
		(uuid "fb72699d-4e75-4adf-9480-f2e2785778ff")
	)
	(segment
		(start 78.74 66.04)
		(end 76.2 63.5)
		(width 0.5)
		(layer "B.Cu")
		(net 2)
		(uuid "43e4a782-fc51-4b31-b336-71d171ec68c0")
	)
	(segment
		(start 78.74 68.58)
		(end 78.74 66.04)
		(width 0.5)
		(layer "B.Cu")
		(net 2)
		(uuid "742e3f6d-383b-4a8d-994e-4935f2e5df72")
	)
	(segment
		(start 76.2 63.5)
		(end 76.2 53.34)
		(width 0.5)
		(layer "B.Cu")
		(net 2)
		(uuid "b01ffd25-5833-4c81-9471-a1575a06f357")
	)
	(segment
		(start 63.5 68.58)
		(end 66.04 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 3)
		(uuid "2e2ca810-ae1c-4724-84d2-edafdb9d8737")
	)
	(segment
		(start 66.04 58.42)
		(end 55.88 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 4)
		(uuid "226b3573-1603-46b9-9966-6a9234192cde")
	)
	(segment
		(start 66.04 53.34)
		(end 66.04 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 4)
		(uuid "7bc43e6d-2d7b-41d8-853c-43b346788095")
	)
	(segment
		(start 66.04 53.34)
		(end 68.58 53.34)
		(width 0.5)
		(layer "B.Cu")
		(net 4)
		(uuid "eec2229a-e191-4843-8ce9-89c5a07f9ca1")
	)
	(segment
		(start 53.34 68.58)
		(end 51.551 66.791)
		(width 0.5)
		(layer "F.Cu")
		(net 5)
		(uuid "b5755ed2-d9dd-4a9d-bae6-d8ae7c8cabb1")
	)
	(segment
		(start 51.551 57.669)
		(end 53.34 55.88)
		(width 0.5)
		(layer "F.Cu")
		(net 5)
		(uuid "d71e5538-88ae-4897-9968-853e28befd64")
	)
	(segment
		(start 51.551 66.791)
		(end 51.551 57.669)
		(width 0.5)
		(layer "F.Cu")
		(net 5)
		(uuid "ed461434-9b49-4569-86f4-873bcb304b4f")
	)
	(segment
		(start 53.34 53.34)
		(end 53.34 55.88)
		(width 0.5)
		(layer "B.Cu")
		(net 5)
		(uuid "0fda121e-1313-4ff4-abee-2eee08187613")
	)
	(segment
		(start 81.28 68.58)
		(end 81.28 71.12)
		(width 0.5)
		(layer "B.Cu")
		(net 6)
		(uuid "278a75b2-177c-468e-b78c-b06e56a05801")
	)
	(segment
		(start 81.28 71.12)
		(end 78.74 71.12)
		(width 0.5)
		(layer "B.Cu")
		(net 6)
		(uuid "b61c62d2-6c34-49a6-bca4-f963b076e673")
	)
	(segment
		(start 90.251 60.400397)
		(end 90.251 69.769)
		(width 0.5)
		(layer "B.Cu")
		(net 7)
		(uuid "6d1f5ccc-27e1-437f-908a-20e1560e3f9f")
	)
	(segment
		(start 87.711 59.609)
		(end 89.459603 59.609)
		(width 0.5)
		(layer "B.Cu")
		(net 7)
		(uuid "79c8c052-fee4-4bcd-bfb4-96a30773350b")
	)
	(segment
		(start 90.251 69.769)
		(end 88.9 71.12)
		(width 0.5)
		(layer "B.Cu")
		(net 7)
		(uuid "8ae370c0-28f0-4069-bd36-2af7b0dff8fa")
	)
	(segment
		(start 86.36 60.96)
		(end 87.711 59.609)
		(width 0.5)
		(layer "B.Cu")
		(net 7)
		(uuid "a0fa09b5-c358-48e4-8110-479469d1eefc")
	)
	(segment
		(start 89.459603 59.609)
		(end 90.251 60.400397)
		(width 0.5)
		(layer "B.Cu")
		(net 7)
		(uuid "f1f62097-27d3-4ead-8033-850dd5338d2a")
	)
	(segment
		(start 86.36 68.58)
		(end 88.9 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 8)
		(uuid "0b7a3a33-7db6-4f18-8b5b-5cbc087e110c")
	)
	(segment
		(start 78.74 60.96)
		(end 86.36 68.58)
		(width 0.5)
		(layer "B.Cu")
		(net 8)
		(uuid "485e2346-9b2d-41bc-8fec-170de284aad8")
	)
	(segment
		(start 73.66 63.5)
		(end 73.66 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 9)
		(uuid "59d91ef4-5bee-4a12-89fb-f64222dfc4d8")
	)
	(segment
		(start 72.39 64.77)
		(end 73.66 63.5)
		(width 0.5)
		(layer "B.Cu")
		(net 9)
		(uuid "70d413e2-1cf9-4cff-ace8-8f6f0c0a9136")
	)
	(segment
		(start 68.58 63.5)
		(end 69.85 64.77)
		(width 0.5)
		(layer "B.Cu")
		(net 9)
		(uuid "c93ec8aa-f913-4461-988c-a97e09386844")
	)
	(segment
		(start 69.85 64.77)
		(end 72.39 64.77)
		(width 0.5)
		(layer "B.Cu")
		(net 9)
		(uuid "f62ad76d-a135-4fc3-a490-8c647cb01a34")
	)
	(segment
		(start 63.5 58.42)
		(end 66.04 60.96)
		(width 0.5)
		(layer "F.Cu")
		(net 10)
		(uuid "65fc7a38-98ad-4916-87e0-9a5ff2398fe0")
	)
	(segment
		(start 55.88 66.04)
		(end 63.5 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 10)
		(uuid "090d305f-45d7-4e15-8ec2-ca73b7121e49")
	)
	(segment
		(start 51.939 62.919686)
		(end 56.438686 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 11)
		(uuid "521ddd4a-be76-4cfe-9926-4b6acf016956")
	)
	(segment
		(start 60.96 55.88)
		(end 60.96 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 11)
		(uuid "b2e56799-1dc2-4fc3-a204-d0955eecdd9b")
	)
	(segment
		(start 53.34 66.04)
		(end 51.939 64.639)
		(width 0.5)
		(layer "B.Cu")
		(net 11)
		(uuid "c9da4046-f46b-419d-bbcd-c89bd3b6378f")
	)
	(segment
		(start 51.939 64.639)
		(end 51.939 62.919686)
		(width 0.5)
		(layer "B.Cu")
		(net 11)
		(uuid "f912e498-b794-41a0-a336-7156df081aa1")
	)
	(segment
		(start 56.438686 58.42)
		(end 60.96 58.42)
		(width 0.5)
		(layer "B.Cu")
		(net 11)
		(uuid "feaaa755-6b12-48f5-a449-a61f7af4876e")
	)
	(segment
		(start 88.9 60.96)
		(end 88.9 66.04)
		(width 0.5)
		(layer "B.Cu")
		(net 12)
		(uuid "dda9ace4-8636-4f14-a7bf-3972277f24b3")
	)
	(segment
		(start 81.28 60.96)
		(end 86.36 66.04)
		(width 0.5)
		(layer "B.Cu")
		(net 13)
		(uuid "5f5965b2-2541-4303-84b6-5649cb17498e")
	)
	(segment
		(start 66.04 63.5)
		(end 63.5 63.5)
		(width 0.5)
		(layer "B.Cu")
		(net 14)
		(uuid "6b0e814c-533a-4662-836e-938ce64b6f3f")
	)
	(segment
		(start 66.04 63.5)
		(end 68.58 60.96)
		(width 0.5)
		(layer "B.Cu")
		(net 14)
		(uuid "a2560d8c-0de0-43e0-b044-3b2f8f9de762")
	)
	(segment
		(start 68.58 60.96)
		(end 71.120001 63.5)
		(width 0.5)
		(layer "B.Cu")
		(net 14)
		(uuid "be6d9bad-e709-406b-b099-b52f681ecc68")
	)
	(embedded_fonts no)
)
