--model ../../samples/scenes/conference/conference.obj
--view-file ../../samples/scenes/conference/conference.view
--light-file ../../samples/scenes/conference/conference.light
--width 128
--height 128
--pack-split-axis
--use-png-ext
--load-assembly rt-llvm.s
--ray-depth 3
--config-file warp.config
--dcacheparams ../../samples/configs/dcacheparams.txt
--icacheparams ../../samples/configs/icacheparams.txt
--usimm-config ../../samples/configs/usimm_configs/gddr5_2ch.cfg
--vi-file ../../samples/configs/usimm_configs/1Gb_x16_amd2GHz.vi
--l1-off
--l2-off
--num-thread-procs 32
--num-icaches 2
--num-icache-banks 8
loading model ../../samples/scenes/conference/conference.obj
loading material file ../../samples/scenes/conference/conference.mtl
43 total materials
282664 total triangles
604956 total vertex normals
vertex min/max = x: (-0.177790, 11.125200) y: (-0.164592, 7.010400) z: (-0.005078, 2.712720)
Starting BVH build.
BVH build complete with 265785 nodes.
before rotations, SAH cost = 40.156631
Scene starts at 66678 (0x00010476)
BVH bounds [-0.177790 -0.164592 -0.005078] [11.125200 7.010400 2.712720]
Loading assembly file rt-llvm.s
Initializing usimm memory module.
---------------------------------------------
-- USIMM: the Utah SImulated Memory Module --
--              Version: 1.3               --
---------------------------------------------
Reading vi file: 1Gb_x16_amd2GHz.vi	
16 Chips per Rank
	 <== Setup time: 14.784 seconds (0:0:14.784) ==>
Creating thread 0...
Thread 0 running cores	0 to	0 ...
	 <== Frame time: 319.446 seconds (0:5:19.446) ==>
System-wide instruction stats (sum/average of all cores):
profile data:
kernel	total calls	total cycles
Data dependence stalls (caused by):
   LOAD        	339070063	(86.820 %)
   FPINVSQRT   	2870433	(0.735 %)
   RAND        	59467	(0.015 %)
   add_s       	3679638	(0.942 %)
   div         	228100	(0.058 %)
   div_s       	25249308	(6.465 %)
   mul_s       	8339118	(2.135 %)
   sub_s       	11048330	(2.829 %)
Number of thread-cycles resource conflicts found when issuing:
   FPMIN       	1330602	(16.795 %)
   FPMAX       	1883693	(23.776 %)
   ATOMIC_INC  	86	(0.001 %)
   FPINVSQRT   	847	(0.011 %)
   RAND        	8	(0.000 %)
   neg_s       	6334	(0.080 %)
   addi        	2	(0.000 %)
   addiu       	147693	(1.864 %)
   addu        	40988	(0.517 %)
   add_s       	640	(0.008 %)
   bal         	478	(0.006 %)
   bc1f        	937078	(11.828 %)
   bc1t        	995942	(12.571 %)
   beq         	7374	(0.093 %)
   beqz        	6953	(0.088 %)
   bnez        	211526	(2.670 %)
   blez        	471088	(5.946 %)
   bne         	9855	(0.124 %)
   cvt_s_w     	1486	(0.019 %)
   c_olt_s     	492137	(6.212 %)
   c_ule_s     	260154	(3.284 %)
   c_ult_s     	5244	(0.066 %)
   div         	636	(0.008 %)
   div_s       	72702	(0.918 %)
   mul         	85	(0.001 %)
   mul_s       	4774	(0.060 %)
   j           	76240	(0.962 %)
   jal         	435213	(5.493 %)
   jr          	481608	(6.079 %)
   ori         	216	(0.003 %)
   sll         	27141	(0.343 %)
   slt         	8224	(0.104 %)
   sltiu       	271	(0.003 %)
   subu        	516	(0.007 %)
   sub_s       	4187	(0.053 %)
   teq         	75	(0.001 %)
   xor_m       	578	(0.007 %)
Dynamic Instruction Mix: (590220168 total)
   FPMIN       	30145380	(5.107 %)
   FPMAX       	30145380	(5.107 %)
   LOAD        	61418088	(10.406 %)
   ATOMIC_INC  	16416	(0.003 %)
   FPINVSQRT   	212964	(0.036 %)
   STORE       	49152	(0.008 %)
   move        	26416060	(4.476 %)
   RAND        	125316	(0.021 %)
   lb          	4660653	(0.790 %)
   lbu         	92796	(0.016 %)
   sb          	370594	(0.063 %)
   neg_s       	129438	(0.022 %)
   addi        	32	(0.000 %)
   addiu       	27317558	(4.628 %)
   addu        	7358438	(1.247 %)
   add_s       	8852838	(1.500 %)
   bal         	64	(0.000 %)
   bc1f        	9048871	(1.533 %)
   bc1t        	9414089	(1.595 %)
   beq         	49143	(0.008 %)
   beqz        	49183	(0.008 %)
   bnez        	1531329	(0.259 %)
   blez        	3369558	(0.571 %)
   bne         	65527	(0.011 %)
   cvt_s_w     	32864	(0.006 %)
   c_olt_s     	11684103	(1.980 %)
   c_ule_s     	6667047	(1.130 %)
   c_ult_s     	111810	(0.019 %)
   div         	16384	(0.003 %)
   div_s       	2060948	(0.349 %)
   lui         	7583291	(1.285 %)
   lw          	30664348	(5.195 %)
   lwc1        	65092344	(11.028 %)
   mfhi        	16384	(0.003 %)
   mflo        	16384	(0.003 %)
   mov_s       	1350008	(0.229 %)
   mtc1        	576850	(0.098 %)
   mul         	16416	(0.003 %)
   mul_s       	62725148	(10.627 %)
   j           	528470	(0.090 %)
   jal         	3336822	(0.565 %)
   jr          	3336854	(0.565 %)
   nop         	18569607	(3.146 %)
   ori         	160	(0.000 %)
   sll         	6050950	(1.025 %)
   slt         	1389422	(0.235 %)
   sltiu       	49151	(0.008 %)
   subu        	98286	(0.017 %)
   sub_s       	54485016	(9.231 %)
   sw          	35498330	(6.014 %)
   swc1        	57407456	(9.726 %)
   teq         	16384	(0.003 %)
   xor_m       	64	(0.000 %)
Issue statistics:
 --Average #threads Issuing each cycle: 17.8669
 --Issue Rate: 55.83%
 --iCache conflicts: 33571695 (3.279006%)
 --thread*cycles of resource conflicts: 7922674 (0.773821%)
 --thread*cycles of data dependence: 390544457 (38.145161%)
 --thread*cycles halted: 1578542 (0.154179%)
 --thread*cycles of issue NOP/other: 18569607 (1.813726%)
Module Utilization

	           FP AddSub:   24.79
	           FP MinMax:   47.11
	          FP Compare:   29.06
	          Int AddSub:   28.31
	              FP Mul:   24.51
	             Int Mul:    0.05
	          FP InvSqrt:    0.67
	              FP Div:    6.49
	     Conversion Unit:    0.10

System-wide L1 stats (sum of all TMs):
L1 OFF!
L1 accesses: 	61467240
L1 hits: 	0
L1 misses: 	61467240
L1 bank conflicts: 	0
L1 stores: 	49152
L1 hit rate: 	0.000000
Hit under miss: 42916310

 -= L2 #0 =-
L2 OFF!
L2 accesses: 	18550930
L2 hits: 	0
L2 misses: 	18412439
L2 stores: 	49152
L2 bank conflicts: 	0
L2 hit rate: 	0.000000
L2 memory faults: 0

Bandwidth numbers for 1000MHz clock (GB/s):
   L1 to register bandwidth: 	 7.684624
   L2 to L1 bandwidth: 		 37.009426
   memory to L2 bandwidth: 	 36.732403

Chip area (mm2):
   Functional units: 	 0.291126
   L1 data caches: 	 0.000000
   L2 data caches: 	 0.000000
   Instruction caches: 	 0.258962
   Localstore units: 	 0.446825
   Register files: 	 0.472528
   ------------------------------
   Total: 		 1.469441

Energy consumption (Joules):
   Functional units: 	 0.003145
   L1 data caches: 	 0.000000
   L2 data caches: 	 0.000000
   Instruction caches: 	 0.007738
   Localstore units: 	 0.001343
   Register files: 	 0.013981
   DRAM: 		 0.465873
   ------------------------------
   Total: 		 0.492080
   Power draw (watts): 	 15.379946

FPS Statistics:
   Total clock cycles: 		 31994923
   FPS assuming 1000MHz clock: 	 31.2550


-------------DRAM stats-------------
Cycles 63989846
-------- Channel 0 Stats-----------
Total Reads Serviced :          3760160
Total Writes Serviced :         5149   
Average Read Latency :          42.97386
Average Read Queue Latency :    10.97386
Average Write Latency :         259.56535
Average Write Queue Latency :   225.56535
Read Page Hit Rate :            0.93380
Write Page Hit Rate :           0.69373
Max write queue length:         4
Max read queue length:          18
Average read queue length:      0.703606
Average column reads per ACT:   15.106504
Single column reads:            57697
Single column reads(%):        1.534429
------------------------------------
-------- Channel 1 Stats-----------
Total Reads Serviced :          3253079
Total Writes Serviced :         5326   
Average Read Latency :          43.11809
Average Read Queue Latency :    11.11809
Average Write Latency :         305.54206
Average Write Queue Latency :   271.54206
Read Page Hit Rate :            0.93128
Write Page Hit Rate :           0.64720
Max write queue length:         5
Max read queue length:          17
Average read queue length:      0.616052
Average column reads per ACT:   14.551582
Single column reads:            52719
Single column reads(%):        1.620588
------------------------------------
-------- Channel 2 Stats-----------
Total Reads Serviced :          7352351
Total Writes Serviced :         4482   
Average Read Latency :          42.49501
Average Read Queue Latency :    10.49501
Average Write Latency :         984.30210
Average Write Queue Latency :   950.30210
Read Page Hit Rate :            0.95292
Write Page Hit Rate :           0.46653
Max write queue length:         5
Max read queue length:          20
Average read queue length:      1.320762
Average column reads per ACT:   21.241035
Single column reads:            87083
Single column reads(%):        1.184424
------------------------------------
-------- Channel 3 Stats-----------
Total Reads Serviced :          3997697
Total Writes Serviced :         4899   
Average Read Latency :          45.90060
Average Read Queue Latency :    13.90060
Average Write Latency :         491.92611
Average Write Queue Latency :   457.92611
Read Page Hit Rate :            0.91597
Write Page Hit Rate :           0.54440
Max write queue length:         5
Max read queue length:          19
Average read queue length:      0.930899
Average column reads per ACT:   11.901095
Single column reads:            85872
Single column reads(%):        2.148037
------------------------------------

#-------------------------------------------------------------------------------------------------
Total memory system power = 14.560842 W
	 <== Total time: 334.244 seconds (0:5:34.244) ==>
